1. What is the square footage of the stone mulch bed shown along the sidewalk as you enter the parking lot?
2. 1065 sqft
3. 543 sqft
4. 1570 sqft
5. 98 sqft
6. The customer would like the identical amount of stone mulch added on the opposite side of the entry way. The price to install stone mulch is $0.25 per sqft. How much will you charge the customer to add the stone mulch?
7. $125
8. $372
9. $403
10. $266
11. How wide are the parking stalls?
12. 4.5ft
13. 15ft
14. 9ft
15. None of the above
16. The 5’ B&B Eastern Red Cedar cost $475. If you charge a 20% markup on each along with $150 to install each. How much will you charge to plant the Eastern Red Cedar’s on the plan?
17. $1,260
18. $8,045
19. $2,880
20. $3,341
21. There is 3,215 **sqft** of sod on the plan. You charge $1.50 per **sqyd**. How much would you charge to provide and install the sod?
22. $535
23. $725
24. $1,237
25. $401
26. The customer would like all trees and shrubs located in the grass areas to have mulch rings. How many mulch rings would be installed?

A.14

B.27

C.31

D. None of the above

1. To what scale is the plan set to?
2. 40
3. 30
4. 20
5. 10
6. What size are the perennials and grasses on the plan?
7. #2 Cont.
8. #1 Cont.
9. 5 gal
10. B&B
11. A group of plants on the plan schedule are Evergreens. Which plant would fall in this category?
12. Quercus Bicolor
13. Ginkgo Biloba
14. Pinus Cembra
15. Hydrangea Paniculata
16. According to the Legend on the plan, what type of edging is called out?
17. Vinyl
18. Brick
19. Shovel cut
20. Aluminum
21. It is important to water the newly install sod using a sprinkler. It is important to not run hoses over parking lots or sidwalks. Each section of sod will require a sprinkler. How many sprinklers will be required to water all the sod?
22. 6
23. 9
24. 3
25. None of the above
26. According to the label on the retaining wall or the legend, what type of wall is the retaining wall made of?
27. Native Boulders
28. Precast concrete block
29. Limestone Boulders
30. Timber
31. The Retaining wall located on the south side of the property located in the plant bed is how many linear feet?
32. 120 LF
33. 54 LF
34. 210 LF
35. 75 LF
36. There is 29,000 sqft of Seeded area. If grass seed is to be applied at a rate of 4lbs per 1000 sqft, how many pounds of seed is needed?
37. 700 lbs
38. 325 lbs
39. 116 lbs
40. 80 lbs
41. It is typical practice to install weed barrier fabric under stone mulch. There is 250 **sqyds** of stone mulch on this project. The rolls of weed fabric are 8’ft x 112’ft. How many rolls will be needed to cover the entire stone mulch area? (9sqft per 1 sqyd)
42. 3 rolls
43. 5.5 rolls
44. 1 roll
45. 2.5 rolls
46. There is 29,000 sqft of seed area that will need to be covered with straw. 1 straw bale covers 500 sqft. How many bales would you bring to the job?
47. 29 bales
48. 58 bales
49. 74 bales
50. None of the above
51. The north parking lot islands contains mulch. The area is 168 sqft. Wood mulch is applied at 3” in depth. How many cubic yards of mulch is required to cover the area? (27 cuft per 1 cuyd)
52. 3 cuyds
53. 1.5 cuyds
54. 4 cuyds
55. 0.5 cuyds
56. How many Allium Summer beauty are called out on the Plant Schedule?
57. 10
58. 5
59. 32
60. 50
61. How many ornamental trees are called out on the plan?
62. 13
63. 5
64. 23
65. 19
66. Under the Contractor Notes it states all disturbed areas to provide Seed, Mulch and one other item. What is that item?
67. Water
68. Sun light
69. Fertilizer
70. None of the above
71. A
72. D
73. C
74. C
75. A
76. B
77. C
78. B
79. C
80. D
81. C
82. C
83. D
84. C
85. D
86. B
87. B
88. D
89. A
90. C